UPDATED 03/04/2024

Sites with loggers:

* LTM E5
* LTM L4
* LTM D6

LOGGER CONFIGURATIONS

* NAME = Serial number of logger
* GROUP = Permanent (for the loggers installed all year) or Camera (for those attached to camera)
* LOGGING INTERVAL = 5 minutes
* START LOGGING = On button push
* SHOW LED = ON
* BLUETOOTH ALWAYS ON = Off
* Temperature and light = enable logging

DEPLOYMENT PROTOCOL

1. Set loggers to settings (see above)
2. Deploy
3. Log the following information:
   * Logger #
   * Location
   * Time deployed
   * Dist. above water

READING OUT LOGGERS:

1. Connect to data logger by pushing the button on the logger while enabling bluetooth on the HOBO connect app
2. Download data, record time downloaded in notebook
3. Once data recorded (MAKE SURE) delete data off the logger
4. Make sure data recording resumes and redeploy logger

\*\*FIGURE OUT BEST WAY TO SAVE DATA IN THE FIELD - excel sheet on the phone

1. Back up data into power bank (depending on how we figure out how to get it off phone. Otherwise will wait till service and email it). Label Data file as: LOGGERNO.SITENO.DATE.TIME.